|  |  |
| --- | --- |
| Observer：\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Date：\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| Location：\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | Time：\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| **Item No.** | **Behaviour to be monitored** | **Safe**  | **At risk**  | **Not observable** |
| **1** | Wear appropriate personal protective equipment in good condition (e.g. safety helmets with y-type chin straps, safety shoes, etc.) |  |  |  |
| **2** | Obtain risk assessment reports and suggestions from competent person before commencement of work |  |  |  |
| **3** | Ensure that equipment for rescue are in good condition (e.g. resuscitator, breathing apparatus) |  |  |  |
| **4** | Check if an effective permit-to-work for confined space is obtained prior to work |  |  |  |
| **5** | Use designated access to and egress from manholes |  |  |  |
| **6** | Provide the working area with good ventilation equipment prior to work |  |  |  |
| **7** | Maintain good communication with the watchman |  |  |  |
| **8** | Wear breathing apparatus and safety harness properly when performing underground piping work |  |  |  |
| **9** | Cancel the permit upon completion of work |  |  |  |
| **10** |  |  |  |  |
| **11** |  |  |  |  |
| **12** |  |  |  |  |
| **13** |  |  |  |  |
| Remark (if any): |
| **Total** |  |  |  |
| **% of safe performance =** |  |  |