|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Observer：\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | Date：\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | |
| Location：\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | Time：\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | | |
| **Item No.** | **Behaviour to be monitored** | | | **Safe** | **At risk** | **Not observable** |
| **1** | Wear appropriate personal protective equipment in good condition (e.g. safety helmet, y-type chin strap, safety shoes, gloves, etc.) | | |  |  |  |
| **2** | Use appropriate working platforms in good condition for work-above-ground (Do not use ladders as working platforms) | | |  |  |  |
| **3** | Wear a full-body safety harness properly and attach it to a secure anchorage ( the hook of the safety harness should be attached to an anchorage above the user to reduce the falling distance) when it is required under legislation and / or contract provision to wear safety harness for working at height | | |  |  |  |
| **4** | Use correct posture and means for manual handling (e.g. keep the back straight, use suitable machinery to aid if necessary) | | |  |  |  |
| **5** | Hang electric cables at high level | | |  |  |  |
| **6** | Use 110V hand-held tools with approved standards | | |  |  |  |
| **7** | Use electric tools with waterproof plugs and wires | | |  |  |  |
| **8** | Wear masks and goggles when handling cement | | |  |  |  |
| **9** | Conduct prior-to-work inspection to plaster mixer and ensure it is safe to operate (including emergency stop button and protective guard ) | | |  |  |  |
| **10** | Store and stack materials properly at designated areas | | |  |  |  |
| **11** | Attach tools with hand straps if there is a risk of falling tools from height when the worker works at height | | |  |  |  |
| **12** |  | | |  |  |  |
| Remark (if any): | | | | | | |
| **Total** | | | |  |  |  |
| **% of safe performance =** | |  | |  | | |